Reference on Literature Data on Foam Stability

S. Ahmed, K. A. Elraies, M. R. Hashmet, and A. S. Hanamertani, “Viscosity models for polymer free CO2 foam fracturing fluid with the effect of surfactant concentration, salinity and shear rate,” *Energies*, vol. 10, no. 12, pp. 12–17, 2017, doi: 10.3390/en10121970.

S. Ahmed, K. A. Elraies, M. R. Hashmet, and M. S. Alnarabiji, “Empirical modeling of the viscosity of supercritical carbon dioxide foam fracturing fluid under different downhole conditions,” *Energies*, vol. 11, no. 4, 2018, doi: 10.3390/en11040782.

P. C. Harris and V. G. Reidenbach, “High-Temperature Rheological Study of Foam Fracturing Fluids.,” *JPT, J. Pet. Technol.*, vol. 39, no. 5, pp. 613–619, 1987, doi: 10.2118/13177-PA.

P. C. Harris, “Chemistry and rheology of borate-crosslinked fluids at temperatures to 300°F,” *JPT, J. Pet. Technol.*, vol. 45, no. 3, pp. 264–269, 1993, doi: 10.2118/24339-PA.

H. Wang, W. Guo, C. Zheng, D. Wang, and H. Zhan, “Effect of Temperature on Foaming Ability and Foam Stability of Typical Surfactants Used for Foaming Agent,” *J. Surfactants Deterg.*, vol. 20, no. 3, pp. 615–622, 2017, doi: 10.1007/s11743-017-1953-9.

Shehab Alzobaidi, Chang Da, Vu Tran, Maša Prodanović, Keith P. Johnston, High temperature ultralow water content carbon dioxide-in-water foam stabilized with viscoelastic zwitterionic surfactants, Journal of Colloid and Interface Science, Volume 488, 2017, Pages 79-91, ISSN 0021-9797.

S. Richard D. Hutchins (SPE), and Matthew J, Miller, (SPE), “A circulating Foam Loop for Evaluating Foam at Conditions of Use,” *SPE Prod. Facil.*, vol. 20, no. 4, pp. 286–294, 2005.

Y. Chen *et al.*, “Switchable nonionic to cationic ethoxylated amine surfactants for CO 2 enhanced oil recovery in high-temperature, high-salinity carbonate reservoirs,” *SPE J.*, vol. 19, no. 2, pp. 249–259, 2014, doi: 10.2118/154222-PA.

Y. Chen *et al.*, “High temperature CO2-in-water foams stabilized with cationic quaternary ammonium surfactants,” *J. Chem. Eng. Data*, vol. 61, no. 8, pp. 2761–2770, 2016, doi: 10.1021/acs.jced.6b00135.

V. Thakore, F. Ren, J. Voytek, H. Wang, J. J. Wang, and Y. Polsky, “High Temperature Stability of Aqueous Foams for Potential Application in Enhanced Geothermal System ( EGS ),” pp. 336–347, 2021.

V. Thakore *et al.*, “High-Temperature Stability of Aqueous Foams as Potential Waterless Hydrofracking Fluid for Geothermal Reservoir Stimulation,” *PROCEEDINGS, 45th Work. Geotherm. Reserv. Eng. Stanford Univ. Stanford, California, Febr. 10-12, 2020 SGP-TR-216*, pp. 1–10, 2020.

P. Zhang *et al.*, “Enhanced stability and high temperature-tolerance of CO2 foam based on a long-chain viscoelastic surfactant for CO2 foam flooding,” *RSC Adv.*, vol. 9, no. 15, pp. 8672–8683, 2019, doi: 10.1039/c9ra00237e.

Y. Wang *et al.*, “The stability study of CO2 foams at high pressure and high temperature,” *J. Pet. Sci. Eng.*, vol. 154, no. April, pp. 234–243, 2017, doi: 10.1016/j.petrol.2017.04.029.

S. M. Lu, “A global review of enhanced geothermal system (EGS),” *Renew. Sustain. Energy Rev.*, vol. 81, no. June 2017, pp. 2902–2921, 2018.

Tyrode, Eric, Aldo Pizzino, and Orlando J. Rojas. "Foamability and foam stability at high pressures and temperatures. I. Instrument validation." *Review of Scientific Instruments* 74.5 (2003): 2925-2932.

E. Rio, W. Drenckhan, A. Salonen, and D. Langevin, “Unusually stable liquid foams,” *Adv. Colloid Interface Sci.*, vol. 205, pp. 74–86, 2014

P. Olasolo, M. C. Juárez, M. P. Morales, S. Damico, and I. A. Liarte, “Enhanced geothermal systems (EGS): A review,” *Renew. Sustain. Energy Rev.*, vol. 56, pp. 133–144, 2016, doi: 10.1016/j.rser.2015.11.031.

C. E. Clark, C. B. Harto, J. L. Sullivan, and M. Q. Wang, “Water Use in the Development and Operation of Geothermal Power Plants,” *Energy Syst. Div. Argonne Natl. Lab.*, no. January, pp. 1–87, 2010, doi: 10.2172/1013997.

I. O. Kohshou *et al.*, “Econ nomic Assessm ment and d Review w of Waterless s Fractu uring Techn nologies s in Sha ale Reso ource Developm ment : A Case Study,” 2017.

W. A. M. Wanniarachchi, P. G. Ranjith, and M. S. A. Perera, “Shale gas fracturing using foam-based fracturing fluid: a review,” *Environ. Earth Sci.*, vol. 76, no. 2, pp. 1–15, 2017, doi: 10.1007/s12665-017-6399-x.

F. K. H., “Comparison of conventional hydrulic and water/nitrogen foam fracturing in two Ohio Devonian shale gas wells,” *Pap. Knowl. . Towar. a Media Hist. Doc.*, no. February, pp. 12–26, 1976.

W. A. M. Wanniarachchi, P. G. Ranjith, M. S. A. Perera, A. Lashin, N. Al Arifi, and J. C. Li, “Current opinions on foam-based hydro-fracturing in deep geological reservoirs,” *Geomech. Geophys. Geo-Energy Geo-Resources*, vol. 1, no. 3–4, pp. 121–134, 2015.

N. Yekeen, E. Padmanabhan, and A. K. Idris, “A review of recent advances in foam-based fracturing fluid application in unconventional reservoirs,” *J. Ind. Eng. Chem.*, vol. 66, pp. 45–71, 2018, doi: 10.1016/j.jiec.2018.05.039.

K. Wilk, “Experimental and simulation studies of energized fracturing fluid effciency in tight gas formations,” *Energies*, vol. 12, no. 23, 2019, doi: 10.3390/en12234465.

S. A. Faroughi, A. J. C. J. Pruvot, and J. McAndrew, “The rheological behavior of energized fluids and foams with application to hydraulic fracturing: Review,” *J. Pet. Sci. Eng.*, vol. 163, no. July 2017, pp. 243–263, 2018, doi: 10.1016/j.petrol.2017.12.051.

H. Wang, W. Guo, C. Zheng, D. Wang, and H. Zhan, “Effect of Temperature on Foaming Ability and Foam Stability of Typical Surfactants Used for Foaming Agent,” *J. Surfactants Deterg.*, vol. 20, no. 3, pp. 615–622, 2017, doi: 10.1007/s11743-017-1953-9.

R. J. B. M. Delahaije, F. J. Lech, and P. A. Wierenga, “Investigating the effect of temperature on the formation and stabilization of ovalbumin foams,” *Food Hydrocoll.*, vol. 91, no. November 2018, pp. 263–274, 2019, doi: 10.1016/j.foodhyd.2019.01.030.

S. Alzobaidi, C. Da, V. Tran, M. Prodanović, and K. P. Johnston, “High temperature ultralow water content carbon dioxide-in-water foam stabilized with viscoelastic zwitterionic surfactants,” *J. Colloid Interface Sci.*, vol. 488, pp. 79–91, 2017.

Q. Lv, Z. Li, B. Li, S. Li, and Q. Sun, “Study of Nanoparticle-Surfactant-Stabilized Foam as a Fracturing Fluid,” *Ind. Eng. Chem. Res.*, vol. 54, no. 38, pp. 9456–9477, 2015, doi: 10.1021/acs.iecr.5b02197.

A. S. Emrani and H. A. Nasr-El-Din, “Stabilizing CO2 foam by use of nanoparticles,” *SPE J.*, vol. 22, no. 2, pp. 494–504, 2017, doi: 10.2118/174254-PA.

C. Fu and N. Liu, “Study of the Synergistic Effect of the Nanoparticle-Surfactant-Polymer System on CO2Foam Apparent Viscosity and Stability at High Pressure and Temperature,” *Energy and Fuels*, vol. 34, no. 11, pp. 13707–13716, 2020.

G. A. Al-muntasheri, E. Advanced, and S. Aramco, “Nanoparticle-Enhanced Hydraulic-Fracturing Fluids : A Review,” no. May, 2017.

S. Ahmed, K. A. Elraies, M. R. Hashmet, and A. S. Hanamertani, “Viscosity models for polymer free CO2 foam fracturing fluid with the effect of surfactant concentration, salinity and shear rate,” *Energies*, vol. 10, no. 12, pp. 12–17, 2017.

S. Ahmed, K. A. Elraies, M. R. Hashmet, and M. S. Alnarabiji, “Empirical modeling of the viscosity of supercritical carbon dioxide foam fracturing fluid under different downhole conditions,” *Energies*, vol. 11, no. 4, 2018.

M. Gu and K. K. Mohanty, “Rheology of polymer-free foam fracturing fluids,” *J. Pet. Sci. Eng.*, vol. 134, pp. 87–96, 2015.

G. I. S. Ranjani and K. Ramamurthy, “Analysis of the Foam Generated Using Surfactant Sodium Lauryl Sulfate,” *Int. J. Concr. Struct. Mater.*, vol. 4, no. 1, pp. 55–62, 2010.

L. Li, G. A. Al-Muntasheri, and F. Liang, “A review of crosslinked fracturing fluids prepared with produced water,” *Petroleum*, vol. 2, no. 4, pp. 313–323, 2016.

M. Ranka, P. Brown, and T. A. Hatton, “Responsive Stabilization of Nanoparticles for Extreme Salinity and High-Temperature Reservoir Applications,” *ACS Appl. Mater. Interfaces*, vol. 7, no. 35, pp. 19651–19658, 2015.

A. Verma, G. Chauhan, and K. Ojha, “Synergistic effects of polymer and bentonite clay on rheology and thermal stability of foam fluid developed for hydraulic fracturing,” *Asia-Pacific J. Chem. Eng.*, vol. 12, no. 6, pp. 872–883, 2017.

M. Simjoo, T. Rezaei, A. Andrianov, and P. L. J. Zitha, “Foam stability in the presence of oil: Effect of surfactant concentration and oil type,” *Colloids Surfaces A Physicochem. Eng. Asp.*, vol. 438, pp. 148–158, 2013.

A. Azdarpour, O. Rahmani, E. Mohammadian, M. Parak, A. R. M. Daud, and R. Junin, “The effects of polymer and surfactant on polymer enhanced foam stability,” *BEIAC 2013 - 2013 IEEE Bus. Eng. Ind. Appl. Colloq.*, no. November 2018.